Farbcodes

The normal mode of the device is its typical operational state when powered on, free from alarms, updates, calibrations, or ongoing configuration changes. LED blinking: In normal mode, the LED will blink 0,5 sec on, 2 sec off to indicate the device's status. The LED colours and patterns will depend on whether the device is included or excluded from the network, as well as whether it is calibrated or not.

Plug S

Green : This LED colour pattern indicates that the device is added (included) in the network. Red SOLID ON: Settings mode: LED solid on

Blue : This LED colour is used for adding (inclusion) or removing (exclusion) of the device from the network.

Red : This LED colour is used for a factory reset.

Yellow : This LED colour is used for calibration of the device (valid for Shutters and Dimmers) Settings in progres: while you're in the setting you want to trigger./Verdana,Geneva,sans-serif;;inherit;;inherit>LED blinking: In settings in progres, the LED will blink 0,1 sec on, 0,1 sec off to indicate the setting being executed. The LED colours and patterns will depend on the selected setting.</font>

Blue : This LED colour indicate that the adding (inclusion) or removing (exclusion) of the device is in progres.

Red : This LED colour Yellow : This LED colour calibration of the device is in progres (valid for Shutters and Dimmers) Settings mode:</font> LED solid on

Blue</font> addingremovingRed</font> factory resetYellow</font> calibrationSettings in progres:</font> while you're in the setting you want to trigger. LED blinking0,1 sec on, 0,1 sec off

Blue</font> addingremovingRed</font> factory reset

Yellow</font> calibration of the device is in progres (valid for Shutters and Dimmers)

Plug S "Device is already owned by another User"

Diese Fehlermeldung erscheint, wenn man versucht, das Device auf der Shelly Cloud zu integrieren. Ursache: die Unique ID des Devices war anfangs nur sechs-stellig und damit zu kurz, um in der gesamten Geräte-Population absolut eindeutig zu sein.

Device ID: 42E6AE (4384430)

Das kann man aber ändern. Wenn der Shelly im lokalen Netz ist, reicht ein http GET auf diese lokale Adresse

http://deviceip/longifyid

Der Shelly Plug S bootet neu und muss wieder in das lokale WLAN übertragen werden. Danach hat er eine lange Unique ID

Device ID: BCFF4D42E6AE (207804698912430)

Das Aufnehmen in die Shelly Cloud funktioniert ohne Probleme.